**************************************************************************
* NOTE: in some cases it's not usefull for very high-bandwidth analyzing *
**************************************************************************
- first of all install CANHackerV2.00.00.exe
- open the USB-CAN and NET-CAN with the baudrate 2400 and enabled hardware handshake ("RTS HS")
  For the SER-CAN you must use 115200 baud.
- and ensure you've read the __WARNING.TXT___ from the USB-CAN driver package:
  "When you've installed the driver, you must call the VBScript regmodify.vbs for each installed port:

   cscript regmodify.vbs COM<x>

  Take a look in the manual for more information."