-- **********************************************************************
-- * IEEE 802.11 Management Information Base
-- **********************************************************************
IEEE802dot11-MIB DEFINITIONS ::= BEGIN
    IMPORTS
        MODULE-IDENTITY, OBJECT-TYPE, 
        NOTIFICATION-TYPE,Integer32, Counter32  FROM SNMPv2-SMI
        DisplayString , MacAddress, RowStatus,
        TruthValue                              FROM SNMPv2-TC
        MODULE-COMPLIANCE, OBJECT-GROUP, 
        NOTIFICATION-GROUP                      FROM SNMPv2-CONF 
        ifIndex                                 FROM RFC1213-MIB;

-- **********************************************************************
-- *  MODULE IDENTITY
-- **********************************************************************
    ieee802dot11 MODULE-IDENTITY
    LAST-UPDATED "9807080000Z"
    ORGANIZATION "IEEE 802.11"
    CONTACT-INFO 
           "WG E-mail: stds-802-11@ieee.org

                Chair: Vic Hayes
               Postal: Lucent Technologies, Inc.
                       Zadelstede 1-10
                       Nieuwegein, Netherlands
                       3431 JZ
                  Tel: +31 30 609 7528
                  Fax: +31 30 231 6233
               E-mail: vichayes@lucent.com

               Editor: Bob O'Hara
               Postal: Informed Technology, Inc.
                       1750 Nantucket Circle, Suite 138
                       Santa Clara, CA 95054 USA
                  Tel: +1 408 986 9596
                  Fax: +1 408 727 2654
               E-mail: bob@informed-technology.com"
    DESCRIPTION
        "The MIB module for IEEE 802.11 entities.
        iso(1).member-body(2).us(840).ieee802dot11(10036)"
    ::= { 1 2 840 10036 }

-- **********************************************************************
-- *  Major sections
-- **********************************************************************
--  Station ManagemenT (SMT) Attributes
    --  DEFINED AS "The SMT object class provides the necessary support at the
    --  station to manage the processes in the station such that the
    --  station may work cooperatively as a part of an IEEE 802.11 network.";

    dot11smt OBJECT IDENTIFIER ::=   {ieee802dot11 1}

      --  dot11smt GROUPS
      --  dot11StationConfigTable            ::= {dot11smt 1}
      --  dot11AuthenticationAlgorithmsTable ::= {dot11smt 2}
      --  dot11WEPDefaultKeysTable           ::= {dot11smt 3}
      --  dot11WEPKeyMappingsTable           ::= {dot11smt 4}
      --  dot11PrivacyTable                  ::= {dot11smt 5}
      --  dot11SMTnotification               ::= {dot11smt 6}

--  MAC Attributes
    --  DEFINED AS "The MAC object class provides the necessary support
    --  for the access control, generation, and verification of frame check
    --  sequences, and proper delivery of valid data to upper layers.";

    dot11mac OBJECT IDENTIFIER ::=   {ieee802dot11 2}

      --  MAC GROUPS
      --  reference IEEE Std 802.1f-1993
         --  dot11OperationTable        ::=    {dot11mac 1}
         --  dot11CountersTable         ::=    {dot11mac 2}
         --  dot11GroupAddressesTable   ::=    {dot11mac 3}

--  Resource Type ID
      dot11res OBJECT IDENTIFIER                ::=   {ieee802dot11 3}
      dot11resAttribute OBJECT IDENTIFIER       ::=   {dot11res 1 }

--  PHY Attributes
    --  DEFINED AS "The PHY object class provides the necessary support
    --  for required PHY operational information that may vary from PHY
    --  to PHY and from STA to STA to be communicated to upper layers."

   dot11phy OBJECT IDENTIFIER ::=   {ieee802dot11 4}

    --  phy GROUPS
    --  dot11PhyOperationTable          ::=  {dot11phy 1}
--  dot11PhyAntennaTable                ::=  {dot11phy 2}
    --  dot11PhyTxPowerTable            ::=  {dot11phy 3}
    --  dot11PhyFHSSTable               ::=  {dot11phy 4}
    --  dot11PhyDSSSTable               ::=  {dot11phy 5}
    --  dot11PhyIRTable                 ::=  {dot11phy 6}
    --  dot11RegDomainsSupportedTable   ::=  {dot11phy 7}
    --  dot11AntennasListTable          ::=  {dot11phy 8}
    --  dot11SupportedDataRatesTxTable  ::=  {dot11phy 9}
    --  dot11SupportedDataRatesRxTable  ::=  {dot11phy 10}


-- **********************************************************************
-- *  Textual conventions from 802 definitions
-- **********************************************************************
    WEPKeytype ::= OCTET STRING (SIZE (0 | 5 | 13))

-- **********************************************************************
-- *  MIB attribute OBJECT-TYPE definitions follow
-- **********************************************************************

-- **********************************************************************
-- *  SMT Station Config  Table
-- **********************************************************************
dot11StationConfigTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11StationConfigEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Station Configuration attributes.  In tablular form to
            allow for multiple instances on an agent."
    ::= {  dot11smt 1 }

dot11StationConfigEntry OBJECT-TYPE
        SYNTAX Dot11StationConfigEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "An entry in the dot11StationConfigTable.  It is
            possible for there to be multiple IEEE 802.11 interfaces
            on one agent, each with its unique MAC address. The
            relationship between an IEEE 802.11 interface and an
            interface in the context of the Internet-standard MIB is
            one-to-one.  As such, the value of an ifIndex object
            instance can be directly used to identify corresponding
            instances of the objects defined herein.  

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."


        INDEX {ifIndex}
    ::= {  dot11StationConfigTable 1 }

Dot11StationConfigEntry ::=
        SEQUENCE {
                dot11StationID                     MacAddress,
                dot11MediumOccupancyLimit          INTEGER,
                dot11CFPollable                    TruthValue,
                dot11CFPPeriod                     INTEGER, 
                dot11CFPMaxDuration                INTEGER,
                dot11AuthenticationResponseTimeOut INTEGER,
                dot11PrivacyOptionImplemented      TruthValue,
                dot11PowerManagementMode           INTEGER,
                dot11DesiredSSID                   OCTET STRING,
                dot11DesiredBSSType                INTEGER,
                dot11OperationalRateSet            OCTET STRING,
                dot11BeaconPeriod                  INTEGER,
                dot11DTIMPeriod                    INTEGER,
                dot11AssociationResponseTimeOut    INTEGER,
                dot11DisassociateReason            INTEGER,
                dot11DisassociateStation           MacAddress,
                dot11DeauthenticateReason          INTEGER,
                dot11DeauthenticateStation         MacAddress,
                dot11AuthenticateFailStatus        INTEGER,
                dot11AuthenticateFailStation       MacAddress }

dot11StationID OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-write
        STATUS deprecated
        DESCRIPTION

            "The purpose of dot11StationID is to allow a manager to identify
            a station for its own purposes.  This attribute provides
            for that eventuality while keeping the true MAC address
            independent.  Its syntax is MAC address and default value
            is the station's assigned, unique MAC address."

    ::= { dot11StationConfigEntry 1 }

dot11MediumOccupancyLimit OBJECT-TYPE
        SYNTAX INTEGER (0..1000)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "This attribute shall indicate the maximum amount of time,
            in TU, that a point coordinator may control the usage of
            the wireless medium without relinquishing control for long
            enough to allow at least one instance of DCF access to the
            medium.  The default value of this attribute shall be 100,
            and the maximum value shall be 1000."

    ::= { dot11StationConfigEntry 2 }

dot11CFPollable OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

        "When this attribute is true, it shall indicate that the STA
        is able to respond to a CF-Poll with a data frame within a
        SIFS time. This attribute shall be false if the STA is not
        able to respond to a CF-Poll with a data frame within a SIFS
        time."

    ::= { dot11StationConfigEntry 3 }

dot11CFPPeriod OBJECT-TYPE
        SYNTAX INTEGER (0..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "The attribute shall describe the number of DTIM intervals
            between the start of CFPs.  It is modified by
            MLME-START.request primitive."

::= {  dot11StationConfigEntry 4 }

dot11CFPMaxDuration OBJECT-TYPE
        SYNTAX INTEGER (0..65535)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

        "The attribute shall describe the maximum duration of the CFP
        in TU that may be generated by the PCF. It is modified by
        MLME-START.request primitive."

::= {  dot11StationConfigEntry 5 }

dot11AuthenticationResponseTimeOut OBJECT-TYPE
        SYNTAX INTEGER (1..4294967295)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "This attribute shall specify the number of TU that a
            responding STA should wait for the next frame in the
            authentication sequence."

    ::= {  dot11StationConfigEntry 6 }

dot11PrivacyOptionImplemented OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "This attribute, when true, shall indicate that the IEEE
             802.11 WEP option is implemented.  The default value of
             this attribute shall be false."

    ::= {  dot11StationConfigEntry 7 }

dot11PowerManagementMode OBJECT-TYPE
                SYNTAX INTEGER { active(1), powersave(2) }
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                        "This attribute shall specify the power management
                         mode of the STA. When set to active, it shall indicate
                         that the station is not in power-save mode. When set
                         to powersave, it shall indicate that the station is
                         in power-save mode. The power management mode is
                         transmitted in all frames according to the rules
                         in  7.1.3.1.7."
        ::= { dot11StationConfigEntry 8 }

dot11DesiredSSID OBJECT-TYPE
                SYNTAX OCTET STRING (SIZE(0..32))
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                        "This attribute reflects the Service Set ID used
                        in the DesiredSSID parameter of the most recent
                        MLME_Scan.request.  This value may be modified
                        by an external management entity and used by the
                        local SME to make decisions about the Scanning process."
        ::= { dot11StationConfigEntry 9 }

dot11DesiredBSSType OBJECT-TYPE
                SYNTAX INTEGER { infrastructure(1), independent(2), any(3) }
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                        "This attribute shall specify the type of BSS the
                         station shall use when scanning for a BSS with which
                         to synchronize. This value is used to filter Probe
                         Response frames and Beacons. When set to infrastructure,
                         the station shall only synchronize with a BSS whose
                         Capability Information field has the ESS subfield set
                         to 1. When set to independent, the station shall only
                         synchronize with a BSS whose Capability Information
                         field has the IBSS subfield set to 1. When set to
                         any, the station may synchronize to either type of
                         BSS."
        ::= { dot11StationConfigEntry 10 }

dot11OperationalRateSet OBJECT-TYPE
                SYNTAX OCTET STRING (SIZE(1..126))
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                        "This attribute shall specify the set of data rates
                         at which the station may transmit data.  Each octet
 contains a value representing a rate.  Each rate
                         shall be within the range from 2 to 127,
                         corresponding to data rates in increments of
                         500 kb/s from 1 Mb/s to 63.5 Mb/s, and shall be
                         supported (as indicated in the supported rates
                         table) for receiving data. This value is reported in
                         transmitted Beacon, Probe Request, Probe Response,
                         Association Request, Association Response,
                         Reassociation Request, and Reassociation Response
                         frames, and is used to determine whether a BSS
                         with which the station desires to synchronize is
                         suitable. It is also used when starting a BSS,
                         as specified in  10.3."
        ::= { dot11StationConfigEntry 11 }

dot11BeaconPeriod OBJECT-TYPE
                SYNTAX INTEGER (1..65535)
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                        "This attribute shall specify the number of TU that a
                         station shall use for scheduling Beacon transmissions.
                         This value is transmitted in Beacon and Probe Response
                         frames."
        ::= { dot11StationConfigEntry 12 }

dot11DTIMPeriod OBJECT-TYPE
                SYNTAX INTEGER(1..255)
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                        "This attribute shall specify the number of beacon
                         intervals that shall elapse between transmission of
                         Beacons frames containing a TIM element whose DTIM
                         Count field is 0. This value is transmitted in
                         the DTIM Period field of Beacon frames."
        ::= { dot11StationConfigEntry 13 }

dot11AssociationResponseTimeOut OBJECT-TYPE
                SYNTAX INTEGER(1..4294967295)
                MAX-ACCESS read-write
                STATUS current
                DESCRIPTION
                        "This attribute shall specify the number of TU that a
                         requesting STA should wait for a response to a
                         transmitted association-request MMPDU."
        ::= { dot11StationConfigEntry 14 }

dot11DisassociateReason OBJECT-TYPE
                SYNTAX INTEGER(0..65535)
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                        "This attribute holds the most recently
                        transmitted Reason Code in a Disassociation
                        frame.  If no Disassociation frame has been
                        transmitted, the value of this attribute shall
                        be 0."

REFERENCE "IEEE Std 802.11-1997, 7.3.1.7"
        ::= { dot11StationConfigEntry 15 }

dot11DisassociateStation OBJECT-TYPE
                SYNTAX MacAddress
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                        "This attribute holds the MAC address from the
                        Address 1 field of the most recently transmitted
                        Disassociation frame.  If no Disassociation
                        frame has been transmitted, the value of this
                        attribute shall be 0."
        ::= { dot11StationConfigEntry 16 }

dot11DeauthenticateReason OBJECT-TYPE
                SYNTAX INTEGER(0..65535)
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                        "This attribute holds the most recently
                        transmitted Reason Code in a Deauthentication
                        frame.  If no Deauthentication frame has been
                        transmitted, the value of this attribute shall
                        be 0."

REFERENCE "IEEE Std 802.11-1997, 7.3.1.7"
        ::= { dot11StationConfigEntry 17 }

dot11DeauthenticateStation OBJECT-TYPE
                SYNTAX MacAddress
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                        "This attribute holds the MAC address from the
                        Address 1 field of the most recently transmitted
                        Deauthentication frame.  If no Deauthentication
                        frame has been transmitted, the value of this
                        attribute shall be 0."
        ::= { dot11StationConfigEntry 18 }

dot11AuthenticateFailStatus OBJECT-TYPE
                SYNTAX INTEGER(0..65535)
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                        "This attribute holds the most recently
                        transmitted Status Code in a failed
                        Authentication frame.  If no failed
                        Authentication frame has been transmitted, the
                        value of this attribute shall be 0."

REFERENCE "IEEE Std 802.11-1997, 7.3.1.9"
        ::= { dot11StationConfigEntry 19 }

dot11AuthenticateFailStation OBJECT-TYPE
                SYNTAX MacAddress
                MAX-ACCESS read-only
                STATUS current
                DESCRIPTION
                        "This attribute holds the MAC address from the
                        Address 1 field of the most recently transmitted
                        failed Authentication frame.  If no failed
                        Authentication frame has been transmitted, the
                        value of this attribute shall be 0."
        ::= { dot11StationConfigEntry 20 }


-- **********************************************************************
-- *    End of dot11StationConfig  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    AuthenticationAlgorithms  TABLE
-- **********************************************************************
dot11AuthenticationAlgorithmsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11AuthenticationAlgorithmsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "This (conceptual) table of attributes shall be a set of
            all the authentication algorithms supported by the
            stations.  The following are the default values and the
            associated algorithm:
                Value = 1: Open System
                Value = 2: Shared Key"
        REFERENCE "IEEE Std 802.11-1997, 7.3.1.1"
    ::= {  dot11smt 2 }

dot11AuthenticationAlgorithmsEntry OBJECT-TYPE
        SYNTAX Dot11AuthenticationAlgorithmsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "An Entry (conceptual row) in the Authentication
            Algorithms Table.  

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."

        INDEX { ifIndex,
              dot11AuthenticationAlgorithmsIndex}
    ::= {  dot11AuthenticationAlgorithmsTable  1 }

Dot11AuthenticationAlgorithmsEntry ::= SEQUENCE {
            dot11AuthenticationAlgorithmsIndex  Integer32,
            dot11AuthenticationAlgorithm        INTEGER,
            dot11AuthenticationAlgorithmsEnable TruthValue }


dot11AuthenticationAlgorithmsIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The auxiliary variable used to identify instances
            of the columnar objects in the Authentication Algorithms Table."
    ::= {  dot11AuthenticationAlgorithmsEntry 1 }

dot11AuthenticationAlgorithm OBJECT-TYPE
        SYNTAX INTEGER {  openSystem (1),   sharedKey (2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

        "This attribute shall be a set of all the authentication
        algorithms supported by the STAs. The following are the
        default values and the associated algorithm.  
        Value = 1: Open System 
        Value = 2: Shared Key"

    ::= {  dot11AuthenticationAlgorithmsEntry 2 }

dot11AuthenticationAlgorithmsEnable  OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

        "This attribute, when true at a station, shall enable the acceptance 
        of the authentication algorithm described in the corresponding table 
        entry in authentication frames received by the station that have odd 
        authentication sequence numbers.  The default value of this attribute 
        shall be 1 for the Open System table entry and 2 for all other table 
        entries."

    ::= {  dot11AuthenticationAlgorithmsEntry 3 }

-- **********************************************************************
-- *    End of AuthenticationAlgorithms  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    WEPDefaultKeys  TABLE
-- **********************************************************************
dot11WEPDefaultKeysTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11WEPDefaultKeysEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Conceptual table for WEP default keys.  This table shall
            contain the four WEP default secret key values
            corresponding to the four possible KeyID values.  The WEP
            default secret keys are logically WRITE-ONLY.  Attempts to
            read the entries in this table shall return unsuccessful
            status and values of null or zero.  The default value of
            each WEP default key shall be null."

        REFERENCE "IEEE Std 802.11-1997, 8.3.2"
    ::= {  dot11smt 3 }

dot11WEPDefaultKeysEntry OBJECT-TYPE
        SYNTAX Dot11WEPDefaultKeysEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "An Entry (conceptual row) in the WEP Default Keys Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."

        INDEX {ifIndex, dot11WEPDefaultKeyIndex}
    ::= {  dot11WEPDefaultKeysTable  1 }

Dot11WEPDefaultKeysEntry ::= SEQUENCE {
            dot11WEPDefaultKeyIndex     INTEGER,
            dot11WEPDefaultKeyValue     WEPKeytype}

dot11WEPDefaultKeyIndex OBJECT-TYPE
        SYNTAX INTEGER (1..4)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The auxiliary variable used to identify instances
            of the columnar objects in the WEP Default Keys Table.
The value of this variable is equal to the WEPDefaultKeyID + 1"
    ::= {  dot11WEPDefaultKeysEntry 1 }

dot11WEPDefaultKeyValue OBJECT-TYPE
        SYNTAX WEPKeytype
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "A WEP default secret key value."
    ::= {  dot11WEPDefaultKeysEntry 2 }

-- **********************************************************************
-- *    End of WEPDefaultKeys  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    WEPKeyMappings  TABLE
-- **********************************************************************
dot11WEPKeyMappingsTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11WEPKeyMappingsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Conceptual table for WEP Key Mappings.  The MIB supports
            the ability to share a separate WEP key for each RA/TA
            pair.  The Key Mappings Table contains zero or one entry
            for each MAC address and contains two fields for each
            entry: WEPOn and the corresponding WEP key.  The WEP key
            mappings are logically WRITE-ONLY.  Attempts to read the
            entries in this table shall return unsuccessful status and
            values of null or zero.  The default value for all WEPOn
            fields is false."
        REFERENCE "IEEE Std 802.11-1997, 8.3.2"
    ::= {  dot11smt 4 }

dot11WEPKeyMappingsEntry OBJECT-TYPE
        SYNTAX Dot11WEPKeyMappingsEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "An Entry (conceptual row) in the WEP Key Mappings Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."

        INDEX {ifIndex, dot11WEPKeyMappingIndex}
    ::= {  dot11WEPKeyMappingsTable  1 }

Dot11WEPKeyMappingsEntry ::= SEQUENCE {
            dot11WEPKeyMappingIndex     Integer32,
            dot11WEPKeyMappingAddress   MacAddress,
            dot11WEPKeyMappingWEPOn     TruthValue,
            dot11WEPKeyMappingValue     WEPKeytype,
            dot11WEPKeyMappingStatus    RowStatus }

dot11WEPKeyMappingIndex OBJECT-TYPE
        SYNTAX Integer32 
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The auxiliary variable used to identify instances
            of the columnar objects in the WEP Key Mappings Table."
    ::= {  dot11WEPKeyMappingsEntry 1 }

dot11WEPKeyMappingAddress OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "The MAC address of the STA for which the values from this
            key mapping entry are to be used."
    ::= {  dot11WEPKeyMappingsEntry 2 }

dot11WEPKeyMappingWEPOn OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "Boolean as to whether WEP is to be used when communicating
            with the dot11WEPKeyMappingAddress STA."
    ::= {  dot11WEPKeyMappingsEntry 3 }

dot11WEPKeyMappingValue OBJECT-TYPE
        SYNTAX WEPKeytype
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "A WEP secret key value."
    ::= {  dot11WEPKeyMappingsEntry 4 }

dot11WEPKeyMappingStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION

            "The status column used for creating, modifying, and
            deleting instances of the columnar objects in the WEP key
            mapping Table."

        DEFVAL {active}
    ::= { dot11WEPKeyMappingsEntry 5 }

-- **********************************************************************
-- *    End of WEPKeyMappings  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PrivacyTable  TABLE
-- **********************************************************************
dot11PrivacyTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PrivacyEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Group containing attributes concerned with IEEE 802.11
            Privacy.  Created as a table to allow multiple
            instantiations on an agent."

    ::= {  dot11smt 5 }

dot11PrivacyEntry OBJECT-TYPE
        SYNTAX Dot11PrivacyEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PrivacyTable Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex}
    ::= {  dot11PrivacyTable 1 }

Dot11PrivacyEntry ::= SEQUENCE {
             dot11PrivacyInvoked                TruthValue,
             dot11WEPDefaultKeyID               INTEGER,
             dot11WEPKeyMappingLength           INTEGER,
             dot11ExcludeUnencrypted            TruthValue,
             dot11WEPICVErrorCount              Counter32,
             dot11WEPExcludedCount              Counter32}


dot11PrivacyInvoked OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

        "When this attribute is true, it shall indicate that the IEEE
        802.11 WEP mechanism is used for transmitting frames of type
        Data. The default value of this attribute shall be false."
    ::= {  dot11PrivacyEntry 1 }

dot11WEPDefaultKeyID  OBJECT-TYPE
        SYNTAX INTEGER (0..3)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "This attribute shall indicate the use of the first,
            second, third, or fourth element of the WEPDefaultKeys
            array when set to values of zero, one, two, or three.  The
            default value of this attribute shall be 0."
        REFERENCE "IEEE Std 802.11-1997, 8.3.2"
    ::= {  dot11PrivacyEntry 2 }

dot11WEPKeyMappingLength  OBJECT-TYPE
        SYNTAX INTEGER (10..4294967295)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The maximum number of tuples that dot11WEPKeyMappings can hold."
        REFERENCE "IEEE Std 802.11-1997, 8.3.2"
    ::= {  dot11PrivacyEntry 3 }

dot11ExcludeUnencrypted  OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

        "When this attribute is true, the STA shall not indicate at
        the MAC service interface received MSDUs that have the WEP
        subfield of the Frame Control field equal to zero. When this
        attribute is false, the STA may accept MSDUs that have the WEP
        subfield of the Frame Control field equal to zero. The default
        value of this attribute shall be false."

    ::= {  dot11PrivacyEntry 4 }

dot11WEPICVErrorCount  OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when a frame is received with the
            WEP subfield of the Frame Control field set to one and the value
            of the ICV as received in the frame does not match the ICV value
            that is calculated for the contents of the received frame."
    ::= {  dot11PrivacyEntry 5 }

dot11WEPExcludedCount  OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "This counter shall increment when a frame is received with the
            WEP subfield of the Frame Control field set to zero and the value
            of dot11ExcludeUnencrypted causes that frame to be discarded."
    ::= {  dot11PrivacyEntry 6 }

-- **********************************************************************
-- *    End of dot11Privacy  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    SMT notification Objects
-- **********************************************************************
    dot11SMTnotification OBJECT IDENTIFIER ::= { dot11smt 6 }

dot11Disassociate NOTIFICATION-TYPE
        OBJECTS { ifIndex, dot11DisassociateReason, dot11DisassociateStation }
        STATUS current
        DESCRIPTION

        "The disassociate notification shall be sent when the STA
        sends a Disassociation frame. The value of the notification
        shall include the MAC address of the MAC to which the Disassociation
        frame was sent and the reason for the disassociation.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."

    ::= { dot11SMTnotification 0 1 }

dot11Deauthenticate NOTIFICATION-TYPE
        OBJECTS { ifIndex, dot11DeauthenticateReason, dot11DeauthenticateStation }
        STATUS current
        DESCRIPTION

        "The deauthenticate notification shall be sent when the STA
        sends a Deauthentication frame. The value of the notification
        shall include the MAC address of the MAC to which the Deauthentication
        frame was sent and the reason for the deauthentication.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."

    ::= { dot11SMTnotification 0 2 }

dot11AuthenticateFail NOTIFICATION-TYPE
        OBJECTS { ifIndex, dot11AuthenticateFailStatus, dot11AuthenticateFailStation }
        STATUS current
        DESCRIPTION

        "The authenticate failure notification shall be sent when the STA
        sends an Authentication frame with a status code other than 
        'successful'. The value of the notification
        shall include the MAC address of the MAC to which the Authentication
        frame was sent and the reason for the authentication failure.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."

::= { dot11SMTnotification 0 3 }


-- **********************************************************************
-- *    End of SMT notification Objects
-- **********************************************************************

-- **********************************************************************
-- *    MAC Attribute Templates
-- **********************************************************************

-- **********************************************************************
-- *    dot11OperationTable  TABLE
-- **********************************************************************
dot11OperationTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11OperationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Group contains MAC attributes pertaining to the operation
            of the MAC.  This has been implemented as a table in order
            to allow for multiple instantiations on an agent."

    ::= {  dot11mac 1 }

dot11OperationEntry OBJECT-TYPE
        SYNTAX Dot11OperationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11OperationEntry Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex}
    ::= {  dot11OperationTable 1 }

Dot11OperationEntry ::= SEQUENCE {
            dot11MACAddress                 MacAddress,
            dot11RTSThreshold               INTEGER,
            dot11ShortRetryLimit            INTEGER,
            dot11LongRetryLimit             INTEGER,
            dot11FragmentationThreshold     INTEGER,
            dot11MaxTransmitMSDULifetime    INTEGER,
            dot11MaxReceiveLifetime         INTEGER,
            dot11ManufacturerID             DisplayString,
            dot11ProductID                  DisplayString}


dot11MACAddress OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
                "Unique MAC Address assigned to the STA."
    ::= {  dot11OperationEntry 1 }

dot11RTSThreshold OBJECT-TYPE
        SYNTAX INTEGER (0..2347)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

        "This attribute shall indicate the number of octets in an MPDU,
        below which an RTS/CTS handshake shall not be performed. An
        RTS/CTS handshake shall be performed at the beginning of any
        frame exchange sequence where the MPDU is of type Data or
        Management, the MPDU has an individual address in the Address1
        field, and the length of the MPDU is greater than
        this threshold. (For additional details, refer to Table 21 in
        9.7.) Setting this attribute to be larger than the maximum
        MSDU size shall have the effect of turning off the RTS/CTS
        handshake for frames of Data or Management type transmitted by
        this STA. Setting this attribute to zero shall have the effect
        of turning on the RTS/CTS handshake for all frames of Data or
        Management type transmitted by this STA. The default value of
        this attribute shall be 2347."

    ::= {  dot11OperationEntry 2 }

dot11ShortRetryLimit OBJECT-TYPE
        SYNTAX INTEGER (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

        "This attribute shall indicate the maximum number of
        transmission attempts of a frame, the length of which is less
        than or equal to dot11RTSThreshold, that shall be made before a
        failure condition is indicated. The default value of this
        attribute shall be 7."

    ::= {  dot11OperationEntry 3 }

dot11LongRetryLimit OBJECT-TYPE
        SYNTAX INTEGER (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

        "This attribute shall indicate the maximum number of
        transmission attempts of a frame, the length of which is
        greater than dot11RTSThreshold, that shall be made before a
        failure condition is indicated. The default value of this
        attribute shall be 4."

    ::= {  dot11OperationEntry 4 }

dot11FragmentationThreshold OBJECT-TYPE
        SYNTAX INTEGER (256..2346)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

        "This attribute shall specify the current maximum size, in
        octets, of the MPDU that may be delivered to the PHY. An MSDU
        shall be broken into fragments if its size exceeds the value
of this attribute after adding MAC headers and trailers. An MSDU or MMPDU shall be fragmented when the resulting frame has an individual address in the Address1 field, and the length of the frame is larger than this threshold. The default value for this attribute shall be the lesser of 2346 or the aMPDUMaxLength of the attached PHY and shall never exceed the lesser of 2346 or the  aMPDUMaxLength of the attached PHY. The value of this attribute shall never be less than 256. "

    ::= {  dot11OperationEntry 5 }

dot11MaxTransmitMSDULifetime OBJECT-TYPE
        SYNTAX INTEGER (1..4294967295)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

        "The MaxTransmitMSDULifetime shall be the elapsed time in TU,
        after the initial transmission of an MSDU, after which further
        attempts to transmit the MSDU shall be terminated. The default
        value of this attribute shall be 512."

    ::= {  dot11OperationEntry 6 }

dot11MaxReceiveLifetime OBJECT-TYPE
        SYNTAX INTEGER (1..4294967295)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "The MaxReceiveLifetime shall be the elapsed time in TU,
            after the initial reception of a fragmented MMPDU or MSDU,
            after which further attempts to reassemble the MMPDU or
            MSDU shall be terminated. The default value shall be
            512."
    ::= {  dot11OperationEntry 7 }

dot11ManufacturerID OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..128))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "The ManufacturerID shall include, at a minimum, the name
            of the manufacturer.  It may include additional
            information at the manufacturer's discretion.  The default
            value of this attribute shall be null."

    ::= {  dot11OperationEntry 8 }

dot11ProductID OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..128))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "The ProductID shall include, at a minimum, an identifier
            that is unique to the manufacturer.  It may include
            additional information at the manufacturer's discretion.
            The default value of this attribute shall be null."

    ::= {  dot11OperationEntry 9 }

-- **********************************************************************
-- *    End of dot11OperationEntry  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11Counters TABLE
-- **********************************************************************
dot11CountersTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11CountersEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Group containing attributes that are MAC counters.
            Implemented as a table to allow for multiple
            instantiations on an agent."

    ::= {  dot11mac 2 }

dot11CountersEntry OBJECT-TYPE
        SYNTAX Dot11CountersEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11CountersEntry Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex}
    ::= {  dot11CountersTable 1 }

Dot11CountersEntry ::= SEQUENCE {
            dot11TransmittedFragmentCount       Counter32,
            dot11MulticastTransmittedFrameCount Counter32,
            dot11FailedCount                    Counter32,
            dot11RetryCount                     Counter32,
            dot11MultipleRetryCount             Counter32,
            dot11FrameDuplicateCount            Counter32,
            dot11RTSSuccessCount                Counter32,
            dot11RTSFailureCount                Counter32,
            dot11ACKFailureCount                Counter32,
            dot11ReceivedFragmentCount          Counter32,
            dot11MulticastReceivedFrameCount    Counter32,
            dot11FCSErrorCount                  Counter32,
            dot11TransmittedFrameCount          Counter32,
            dot11WEPUndecryptableCount          Counter32 }

dot11TransmittedFragmentCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "This counter shall be incremented for an acknowledged MPDU
            with an individual address in the address 1 field or an MPDU
            with a multicast address in the address 1 field of type Data
            or Management."

    ::= {  dot11CountersEntry 1 }

dot11MulticastTransmittedFrameCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            " This counter shall increment only when the multicast bit
            is set in the destination MAC address of a successfully
            transmitted MSDU.  When operating as a STA in an ESS, where
            these frames are directed to the AP, this implies having
            received an acknowledgment to all associated MPDUs. "

    ::= {  dot11CountersEntry 2 }

dot11FailedCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

        "This counter shall increment when an MSDU is not transmitted
        successfully due to the number of transmit attempts exceeding
        either the  dot11ShortRetryLimit or dot11LongRetryLimit. "

    ::= {  dot11CountersEntry 3 }

dot11RetryCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "This counter shall increment when an MSDU is successfully
            transmitted after one or more retransmissions."
    ::= {  dot11CountersEntry 4 }

dot11MultipleRetryCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "This counter shall increment when an MSDU is successfully
            transmitted after more than one retransmission."

    ::= {  dot11CountersEntry 5 }

dot11FrameDuplicateCount  OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "This counter shall increment when a frame is received
            that the Sequence Control field indicates is a
            duplicate."

    ::= {  dot11CountersEntry 6 }

dot11RTSSuccessCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "This counter shall increment when a CTS is received in
            response to an RTS."
        ::= {  dot11CountersEntry 7 }

dot11RTSFailureCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION


        "This counter shall increment when a CTS is not received in
        response to an RTS."

    ::= { dot11CountersEntry 8 }

dot11ACKFailureCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "This counter shall increment when an ACK is not received
            when expected."

    ::= {  dot11CountersEntry 9 }

dot11ReceivedFragmentCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "This counter shall be incremented for each successfully
            received MPDU of type Data or Management."

    ::= {  dot11CountersEntry 10 }

dot11MulticastReceivedFrameCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "This counter shall increment when a MSDU is received
            with the multicast bit set in the destination
            MAC address."
    ::= {  dot11CountersEntry 11 }

dot11FCSErrorCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "This counter shall increment when an FCS error is
            detected in a received MPDU."

    ::= {  dot11CountersEntry 12 }

dot11TransmittedFrameCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

"This counter shall increment for each successfully transmitted MSDU."

    ::= {  dot11CountersEntry 13 }

dot11WEPUndecryptableCount OBJECT-TYPE
        SYNTAX Counter32
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

        "This counter shall increment when a frame is received with
        the WEP subfield of the Frame Control field set to one and the
        WEPOn value for the key mapped to the TA's MAC address
        indicates that the frame should not have been encrypted or
        that frame is discarded due to the receiving STA not
        implementing the privacy option."

    ::= { dot11CountersEntry 14 }

-- **********************************************************************
-- *    End of dot11CountersEntry  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    GroupAddresses  TABLE
-- **********************************************************************
dot11GroupAddressesTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11GroupAddressesEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "A conceptual table containing a set of MAC addresses
            identifying the multicast addresses for which this STA
            will receive frames.  The default value of this attribute
            shall be null."

    ::= {  dot11mac 3 }

dot11GroupAddressesEntry OBJECT-TYPE
        SYNTAX Dot11GroupAddressesEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An Entry (conceptual row) in the Group Addresses Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex, dot11GroupAddressesIndex}
    ::= {  dot11GroupAddressesTable  1 }

Dot11GroupAddressesEntry ::= SEQUENCE {
            dot11GroupAddressesIndex    Integer32,
            dot11Address                MacAddress,
            dot11GroupAddressesStatus   RowStatus}

dot11GroupAddressesIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The auxiliary variable used to identify instances
            of the columnar objects in the Group Addresses Table."
    ::= {  dot11GroupAddressesEntry 1 }

dot11Address OBJECT-TYPE
        SYNTAX MacAddress
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION
            "MAC address identifying a multicast addresses
            from which this STA will receive frames."
    ::= {  dot11GroupAddressesEntry 2 }

dot11GroupAddressesStatus OBJECT-TYPE
        SYNTAX RowStatus
        MAX-ACCESS read-create
        STATUS current
        DESCRIPTION

            "The status column used for creating, modifying, and
            deleting instances of the columnar objects in the Group
            Addresses Table."

        DEFVAL {active}
    ::= {  dot11GroupAddressesEntry 3 }
-- **********************************************************************
-- *    End of GroupAddress  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    Resource Type Attribute Templates
-- **********************************************************************
dot11ResourceTypeIDName OBJECT-TYPE
        SYNTAX DisplayString (SIZE(4))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "Contains the name of the Resource Type ID managed object.
            The attribute is read-only and always contains the value
            RTID.  This attribute value shall not be used as a naming
            attribute for any other managed object class."

        REFERENCE "IEEE Std 802.1F-1993,  A.7"
        DEFVAL {"RTID"}
    ::= {  dot11resAttribute 1 }

-- **********************************************************************
-- *    dot11ResourceInfo  TABLE
-- **********************************************************************
dot11ResourceInfoTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11ResourceInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Provides a means of indicating, in data readable from a
            managed object, information that identifies the source of
            the implementation."

        REFERENCE "IEEE Std 802.1F-1993,  A.7"
    ::= {  dot11resAttribute 2 }

dot11ResourceInfoEntry OBJECT-TYPE
        SYNTAX Dot11ResourceInfoEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11ResourceInfo Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex}
    ::= {  dot11ResourceInfoTable 1 }

Dot11ResourceInfoEntry ::= SEQUENCE {
            dot11manufacturerOUI             OCTET STRING,
            dot11manufacturerName            DisplayString,
            dot11manufacturerProductName     DisplayString,
            dot11manufacturerProductVersion  DisplayString}


dot11manufacturerOUI OBJECT-TYPE
        SYNTAX OCTET STRING (SIZE(3))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Takes the value of an organizationally unique identifier."
    ::= {  dot11ResourceInfoEntry 1 }

dot11manufacturerName OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..128))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "A printable string used to identify the manufacturer of the
            resource.  Maximum string length is 128 octets."
    ::= {  dot11ResourceInfoEntry 2 }

dot11manufacturerProductName OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..128))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "A printable string used to identify the manufacturer's product
            name of the resource.  Maximum string length is 128 octets."
    ::= {  dot11ResourceInfoEntry 3 }

dot11manufacturerProductVersion OBJECT-TYPE
        SYNTAX DisplayString (SIZE(0..128))
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "Printable string used to identify the manufacturer's product
            version of the resource.  Maximum string length is 128 octets."
    ::= {  dot11ResourceInfoEntry 4 }

-- **********************************************************************
-- *    End of dot11ResourceInfo  TABLE
-- **********************************************************************

-- **********************************************************************
-- *   PHY Attribute Templates
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyOperation  TABLE
-- **********************************************************************
dot11PhyOperationTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyOperationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

        "PHY level attributes concerned with
        operation.  Implemented as a table indexed on
        ifIndex to allow for multiple instantiations on an
        Agent."

    ::= {  dot11phy 1 }

dot11PhyOperationEntry OBJECT-TYPE
        SYNTAX Dot11PhyOperationEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyOperation Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex}
    ::= {  dot11PhyOperationTable 1 }

Dot11PhyOperationEntry ::= SEQUENCE {
            dot11PHYType            INTEGER,
            dot11CurrentRegDomain   Integer32,
            dot11TempType           INTEGER }

dot11PHYType OBJECT-TYPE
        SYNTAX INTEGER {fhss(1), dsss(2), irbaseband(3)}
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

        "This is an 8-bit integer value that identifies the PHY type
        supported by the attached PLCP and PMD. Currently defined
        values and their corresponding PHY types are:

        FHSS 2.4 GHz = 01 , DSSS 2.4 GHz = 02, IR Baseband = 03"

    ::= {  dot11PhyOperationEntry 1 }

dot11CurrentRegDomain OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "The current regulatory domain this instance of the PMD is
            supporting.  This object corresponds to one of the
            RegDomains listed in dot11RegDomainsSupported."

    ::= {   dot11PhyOperationEntry 2 }

dot11TempType OBJECT-TYPE
        SYNTAX INTEGER {tempType1(1), tempType2(2) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

        "There are different operating temperature requirements
        dependent on the anticipated environmental conditions. This
        attribute describes the current PHY's operating temperature
        range capability. Currently defined values and their
        corresponding temperature ranges are:

        Type 1 = X'01'-Commercial range of 0 to 40 degrees C,

        Type 2 = X'02'-Industrial range of -30 to 70 degrees C."

    ::= {   dot11PhyOperationEntry 3 }




-- **********************************************************************
-- *    End of dot11PhyOperation  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyAntenna  TABLE
-- **********************************************************************
dot11PhyAntennaTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyAntennaEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Group of attributes for PhyAntenna.  Implemented as a
            table indexed on ifIndex to allow for multiple instances on
            an agent."

    ::= {  dot11phy 2}

dot11PhyAntennaEntry OBJECT-TYPE
        SYNTAX Dot11PhyAntennaEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyAntenna Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex}
    ::= {  dot11PhyAntennaTable 1 }

Dot11PhyAntennaEntry ::= SEQUENCE {
             dot11CurrentTxAntenna  Integer32,
             dot11DiversitySupport  INTEGER,
             dot11CurrentRxAntenna  Integer32 }

dot11CurrentTxAntenna OBJECT-TYPE
        SYNTAX Integer32 (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "The current antenna being used to transmit.  This value
        is one of the values appearing in
        dot11SupportedTxAntenna. This may be used by a management agent to control which antenna is used for transmission. "

    ::= {  dot11PhyAntennaEntry 1 }

dot11DiversitySupport OBJECT-TYPE
        SYNTAX INTEGER {fixedlist(1), notsupported(2), dynamic(3)}
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

        "This implementation's support for diversity, encoded as:

        X'01'-diversity is available and is performed over the fixed
            list of antennas defined in dot11DiversitySelectionRx.

        X'02'-diversity is not supported.

        X'03'-diversity is supported and control of diversity is also
            available, in which case the attribute 
            dot11DiversitySelectionRx can be dynamically modified by the
            LME."
    ::= {  dot11PhyAntennaEntry 2 }

dot11CurrentRxAntenna OBJECT-TYPE
        SYNTAX Integer32 (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

"The current antenna being used to receive, if the dot11 DiversitySupport indicates that diversity is not supported.  The selected antenna shall be one of the antennae marked for receive in the dot11AntennasListTable. "

    ::= {  dot11PhyAntennaEntry 3 }

-- **********************************************************************
-- *    End of dot11PhyAntenna  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyTxPower  TABLE
-- **********************************************************************
dot11PhyTxPowerTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyTxPowerEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Group of attributes for dot11PhyTxPowerTable.  Implemented
            as a table indexed on STA ID to allow for multiple
            instances on an Agent."

    ::= {  dot11phy 3}

dot11PhyTxPowerEntry OBJECT-TYPE
        SYNTAX Dot11PhyTxPowerEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyTxPower Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex}
    ::= {  dot11PhyTxPowerTable 1 }

Dot11PhyTxPowerEntry ::= SEQUENCE {
            dot11NumberSupportedPowerLevels  INTEGER,
            dot11TxPowerLevel1               INTEGER,
            dot11TxPowerLevel2               INTEGER,
            dot11TxPowerLevel3               INTEGER,
            dot11TxPowerLevel4               INTEGER,
            dot11TxPowerLevel5               INTEGER,
            dot11TxPowerLevel6               INTEGER,
            dot11TxPowerLevel7               INTEGER,
            dot11TxPowerLevel8               INTEGER,
            dot11CurrentTxPowerLevel         INTEGER}

dot11NumberSupportedPowerLevels OBJECT-TYPE
        SYNTAX INTEGER (1..8)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The number of power levels supported by the PMD.
            This attribute can have a value of 1 to 8."
    ::= {  dot11PhyTxPowerEntry 1 }

dot11TxPowerLevel1 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL1 in mW.
            This is also the default power level."
    ::= {   dot11PhyTxPowerEntry 2 }

dot11TxPowerLevel2 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL2 in mW."
    ::= {   dot11PhyTxPowerEntry 3 }

dot11TxPowerLevel3 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL3 in mW."
    ::= {   dot11PhyTxPowerEntry 4 }

dot11TxPowerLevel4 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL4 in mW."
    ::= {   dot11PhyTxPowerEntry 5 }

dot11TxPowerLevel5 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL5 in mW."
    ::= {   dot11PhyTxPowerEntry 6 }

dot11TxPowerLevel6 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL6 in mW."
    ::= {   dot11PhyTxPowerEntry 7 }

dot11TxPowerLevel7 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL7 in mW."
    ::= {   dot11PhyTxPowerEntry 8 }

dot11TxPowerLevel8 OBJECT-TYPE
        SYNTAX INTEGER (0..10000)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The transmit output power for LEVEL8 in mW."
    ::= {   dot11PhyTxPowerEntry 9 }

dot11CurrentTxPowerLevel OBJECT-TYPE
        SYNTAX INTEGER (1..8)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "The TxPowerLevel N currently being used to transmit data.
            Some PHYs also use this value to determine the receiver
            sensitivity requirements for CCA."

    ::= {   dot11PhyTxPowerEntry 10 }

-- **********************************************************************
-- *    End of dot11PhyTxPower  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyFHSS  TABLE
-- **********************************************************************
dot11PhyFHSSTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyFHSSEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Group of attributes for dot11PhyFHSSTable.  Implemented as a
            table indexed on STA ID to allow for multiple instances on
            an Agent."

    ::= {  dot11phy 4 }

dot11PhyFHSSEntry OBJECT-TYPE
        SYNTAX Dot11PhyFHSSEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyFHSS Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex}
    ::= {  dot11PhyFHSSTable 1 }

Dot11PhyFHSSEntry ::= SEQUENCE {
             dot11HopTime               INTEGER,
             dot11CurrentChannelNumber  INTEGER,
             dot11MaxDwellTime          INTEGER,
             dot11CurrentDwellTime      INTEGER,
             dot11CurrentSet            INTEGER,
             dot11CurrentPattern        INTEGER,
             dot11CurrentIndex          INTEGER}

dot11HopTime OBJECT-TYPE
        SYNTAX INTEGER (224)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The time in microseconds for the PMD to change from
            channel 2 to channel 80"
    ::= {   dot11PhyFHSSEntry 1 }

dot11CurrentChannelNumber OBJECT-TYPE
        SYNTAX INTEGER (0..99)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
        "The current channel number of the frequency output by the RF
        synthesizer"
    ::= {   dot11PhyFHSSEntry 2 }

dot11MaxDwellTime OBJECT-TYPE
        SYNTAX INTEGER (1..65535)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The maximum time in TU that the transmitter
            is permitted to operate on a single channel."
    ::= {   dot11PhyFHSSEntry 3 }

dot11CurrentDwellTime OBJECT-TYPE
        SYNTAX INTEGER (1..65535)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current time in TU that the transmitter shall operate
            on a single channel, as set by the MAC.  Default is 19 TU."
    ::= {   dot11PhyFHSSEntry 4 }

dot11CurrentSet OBJECT-TYPE
        SYNTAX INTEGER (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current set of patterns the PHY
            LME is using to determine the hopping sequence. "
    ::= {   dot11PhyFHSSEntry 5 }

dot11CurrentPattern OBJECT-TYPE
        SYNTAX INTEGER (0..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current pattern the PHY LME is
            using to determine the hop sequence."
    ::= {   dot11PhyFHSSEntry 6 }

dot11CurrentIndex OBJECT-TYPE
        SYNTAX INTEGER (1..255)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "The current index value the PHY LME is using to determine
            the CurrentChannelNumber."

    ::= {   dot11PhyFHSSEntry 7 }

-- **********************************************************************
-- *    End of dot11PhyFHSS  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyDSSSEntry  TABLE
-- **********************************************************************
dot11PhyDSSSTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyDSSSEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Entry of attributes for dot11PhyDSSSEntry.  Implemented as a
            table indexed on ifIndex allow for multiple instances on
            an Agent."

    ::= {  dot11phy 5 }

dot11PhyDSSSEntry OBJECT-TYPE
        SYNTAX Dot11PhyDSSSEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyDSSSEntry Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex}
    ::= {  dot11PhyDSSSTable 1 }

Dot11PhyDSSSEntry ::= SEQUENCE {
             dot11CurrentChannel    INTEGER,
             dot11CCAModeSupported  INTEGER,
             dot11CurrentCCAMode    INTEGER,
             dot11EDThreshold       Integer32}

dot11CurrentChannel OBJECT-TYPE
        SYNTAX INTEGER (1..14)
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current operating frequency channel of the DSSS
            PHY. Valid channel numbers are as defined in 15.4.6.2"
    ::= {   dot11PhyDSSSEntry 1 }

dot11CCAModeSupported OBJECT-TYPE
        SYNTAX INTEGER (1..7)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "dot11CCAModeSupported is a bit-significant value, representing all of the CCA modes supported by the PHY.  Valid values are:

            energy detect only (ED_ONLY) = 01,
                carrier sense only (CS_ONLY) = 02,
                carrier sense and energy detect (ED_and_CS)= 04

or the logical sum of any of these values."
    ::= {   dot11PhyDSSSEntry 2 }

dot11CurrentCCAMode OBJECT-TYPE
        SYNTAX INTEGER {edonly(1), csonly(2), edandcs(4)}
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current CCA method in operation.   Valid values are:
                energy detect only (edonly) = 01,
                carrier sense only (csonly) = 02,
                carrier sense and energy detect (edandcs)= 04."
::= {   dot11PhyDSSSEntry 3 }

dot11EDThreshold OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The current Energy Detect Threshold being used by the DSSS PHY."
    ::= {   dot11PhyDSSSEntry 4 }

-- **********************************************************************
-- *    End of dot11PhyDSSSEntry  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11PhyIR  TABLE
-- **********************************************************************
dot11PhyIRTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11PhyIREntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Group of attributes for dot11PhyIRTable.  Implemented as a
            table indexed on ifIndex to allow for multiple instances on
            an Agent."

    ::= {  dot11phy 6 }

dot11PhyIREntry OBJECT-TYPE
        SYNTAX Dot11PhyIREntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11PhyIR Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex}
    ::= {  dot11PhyIRTable 1 }

Dot11PhyIREntry ::= SEQUENCE {
             dot11CCAWatchdogTimerMax       Integer32,
             dot11CCAWatchdogCountMax       Integer32,
             dot11CCAWatchdogTimerMin       Integer32,
             dot11CCAWatchdogCountMin       Integer32}

dot11CCAWatchdogTimerMax OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "This parameter, together with CCAWatchdogCountMax,
            determines when energy detected in the channel can be
            ignored."

    ::= {   dot11PhyIREntry 1 }

dot11CCAWatchdogCountMax OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "This parameter, together with CCAWatchdogTimerMax,
            determines when energy detected in the channel can be
            ignored."

    ::= {   dot11PhyIREntry 2 }

dot11CCAWatchdogTimerMin OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "The minimum value to which CCAWatchdogTimerMax can be
            set."

    ::= {   dot11PhyIREntry 3 }

dot11CCAWatchdogCountMin OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION
            "The minimum value to which CCAWatchdogCount can be set."
    ::= {   dot11PhyIREntry 4 }

-- **********************************************************************
-- *    End of dot11PhyIR  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11RegDomainsSupported  TABLE
-- **********************************************************************
dot11RegDomainsSupportedTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11RegDomainsSupportEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "There are different operational requirements dependent on
            the regulatory domain.  This attribute list describes the
            regulatory domains the PLCP and PMD support in this
            implementation.  Currently defined values and their
            corresponding Regulatory Domains are:

            FCC (USA) = X'10', DOC (Canada) = X'20', ETSI (most of
            Europe) = X'30', Spain = X'31', France = X'32', MKK
            (Japan) = X'40' "

    ::= {   dot11phy 7}

dot11RegDomainsSupportEntry OBJECT-TYPE
        SYNTAX Dot11RegDomainsSupportEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11RegDomainsSupport Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex, dot11RegDomainsSupportIndex}
    ::= {  dot11RegDomainsSupportedTable 1 }

Dot11RegDomainsSupportEntry ::= SEQUENCE {
             dot11RegDomainsSupportIndex    Integer32,
             dot11RegDomainsSupportValue    INTEGER}

dot11RegDomainsSupportIndex OBJECT-TYPE
        SYNTAX Integer32
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The auxiliary variable used to identify instances
            of the columnar objects in the RegDomainsSupport Table."
    ::= {  dot11RegDomainsSupportEntry 1 }

dot11RegDomainsSupportValue OBJECT-TYPE

        SYNTAX INTEGER {fcc(16), doc(32), etsi(48), spain (49), france
        (50), mkk (64) }
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "There are different operational requirements dependent on
            the regulatory domain.  This attribute list describes the
            regulatory domains the PLCP and PMD support in this
            implementation.  Currently de- fined values and their
            corresponding Regulatory Domains are:

            FCC (USA) = X'10', DOC (Canada) = X'20', ETSI (most of
            Europe) = X'30', Spain = X'31', France = X'32', MKK
            (Japan) = X'40' "
    ::= {  dot11RegDomainsSupportEntry 2 }

-- **********************************************************************
-- *    End of dot11RegDomainsSupported  TABLE
-- **********************************************************************

-- **********************************************************************
-- *    dot11AntennasList  TABLE
-- **********************************************************************
dot11AntennasListTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11AntennasListEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
"This table represents the list of antennae.  An antenna can be marked to be capable of transmitting, receiving, and/or for participation in receive diversity.  Each entry in this table represents a single antenna with its properties.  The maximum number of antennae that can be contained in this table is 255."
    ::= {   dot11phy 8 }

dot11AntennasListEntry OBJECT-TYPE
        SYNTAX Dot11AntennasListEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "An entry in the dot11AntennasListTable, representing the properties of a single antenna.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."
        INDEX {ifIndex, dot11AntennaListIndex}
    ::= {  dot11AntennasListTable 1 }

Dot11AntennasListEntry ::= SEQUENCE {
             dot11AntennaListIndex     Integer32,
             dot11SupportedTxAntenna   TruthValue,
             dot11SupportedRxAntenna   TruthValue,
             dot11DiversitySelectionRx TruthValue }

dot11AntennaListIndex OBJECT-TYPE
        SYNTAX Integer32 (1..255)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The unique index of an antenna which is used to identify the columnar objects in the dot11AntennasList Table."
    ::= {  dot11AntennasListEntry 1 }

dot11SupportedTxAntenna OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "When true, this object indicates that the antenna represented by dot11AntennaIndex can be used as a transmit antenna."

    ::= {  dot11AntennasListEntry 2 }

dot11SupportedRxAntenna OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "When true, this object indocates that the antenna represented by the dot11AntennaIndex xan be used as a receive antenna."

    ::= {  dot11AntennasListEntry 3 }

dot11DiversitySelectionRx OBJECT-TYPE
        SYNTAX TruthValue
        MAX-ACCESS read-write
        STATUS current
        DESCRIPTION

            "When true, this object indicates that the antenna represented by dot11AntennaIndex can be used for receive diversity.  This object may only be true if the antenna can be used as a receive antenna, as indicated by dot11SupportedRxAntenna."

    ::= {  dot11AntennasListEntry 4 }

-- **********************************************************************
-- *    End of dot11AntennasList  TABLE
-- **********************************************************************


-- **********************************************************************
-- *    SupportedDataRatesTx  TABLE
-- **********************************************************************
dot11SupportedDataRatesTxTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11SupportedDataRatesTxEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "The Transmit bit rates supported by the PLCP and PMD,
            represented by a count from X'02-X'7f, corresponding to data
            rates in increments of 500Kb/s from 1 Mb/s to 63.5 Mb/s subject
            to limitations of each individual PHY."

    ::= {  dot11phy 9 }

dot11SupportedDataRatesTxEntry OBJECT-TYPE
        SYNTAX Dot11SupportedDataRatesTxEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "An Entry (conceptual row) in the dot11SupportedDataRatesTx
            Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."

        INDEX {ifIndex, dot11SupportedDataRatesTxIndex}

    ::= {  dot11SupportedDataRatesTxTable  1 }

Dot11SupportedDataRatesTxEntry ::= SEQUENCE {
            dot11SupportedDataRatesTxIndex  Integer32,
            dot11SupportedDataRatesTxValue  Integer32}

dot11SupportedDataRatesTxIndex OBJECT-TYPE
        SYNTAX Integer32 (1..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "Index object which identifies which data rate to access.
            Range is 1..8."

    ::= {  dot11SupportedDataRatesTxEntry 1 }

dot11SupportedDataRatesTxValue OBJECT-TYPE
        SYNTAX Integer32 (2..127)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION

            "The Transmit bit rates supported by the PLCP and PMD,
            represented by a count from X'02-X'7f, corresponding to data
            rates in increments of 500Kb/s from 1 Mb/s to 63.5 Mb/s subject
            to limitations of each individual PHY."

    ::= {  dot11SupportedDataRatesTxEntry 2 }

-- **********************************************************************
-- *    End of dot11SupportedDataRatesTx  TABLE
-- **********************************************************************


-- **********************************************************************
-- *    SupportedDataRatesRx  TABLE
-- **********************************************************************
dot11SupportedDataRatesRxTable OBJECT-TYPE
        SYNTAX SEQUENCE OF Dot11SupportedDataRatesRxEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "The receive bit rates supported by the PLCP and PMD,
            represented by a count from X'002-X'7f, corresponding to data
            rates in increments of 500Kb/s from 1 Mb/s to 63.5 Mb/s."

    ::= {  dot11phy 10 }

dot11SupportedDataRatesRxEntry OBJECT-TYPE
        SYNTAX Dot11SupportedDataRatesRxEntry
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION

            "An Entry (conceptual row) in the
        dot11SupportedDataRatesRx Table.

            ifIndex - Each 802.11 interface is represented by an
            ifEntry.  Interface tables in this MIB module are indexed
            by ifIndex."

        INDEX {ifIndex, dot11SupportedDataRatesRxIndex}

    ::= {  dot11SupportedDataRatesRxTable  1 }

Dot11SupportedDataRatesRxEntry ::= SEQUENCE {
            dot11SupportedDataRatesRxIndex  Integer32,
            dot11SupportedDataRatesRxValue  Integer32}

dot11SupportedDataRatesRxIndex OBJECT-TYPE
        SYNTAX Integer32 (1..8)
        MAX-ACCESS not-accessible
        STATUS current
        DESCRIPTION
            "Index object which identifies which data rate to access.
            Range is 1..8."
    ::= {  dot11SupportedDataRatesRxEntry 1 }

dot11SupportedDataRatesRxValue OBJECT-TYPE
        SYNTAX Integer32 (2..127)
        MAX-ACCESS read-only
        STATUS current
        DESCRIPTION
            "The receive bit rates supported by the PLCP and PMD,
            represented by a count from X'02-X'7f, corresponding to data
            rates in increments of 500Kb/s from 1 Mb/s to 63.5 Mb/s."
    ::= {  dot11SupportedDataRatesRxEntry 2 }

-- **********************************************************************
-- *    End of dot11SupportedDataRatesRx  TABLE
-- **********************************************************************

-- **********************************************************************
-- *   conformance information
-- **********************************************************************

dot11Conformance  OBJECT IDENTIFIER ::= { ieee802dot11 5 }
dot11Groups  OBJECT IDENTIFIER ::= { dot11Conformance 1 }
dot11Compliances  OBJECT IDENTIFIER ::= { dot11Conformance 2 }

-- **********************************************************************
-- *   compliance statements
-- **********************************************************************
dot11Compliance MODULE-COMPLIANCE
        STATUS  current
        DESCRIPTION
            "The compliance statement for SNMPv2 entities
            that implement the IEEE 802.11 MIB."

  MODULE  -- this module
    MANDATORY-GROUPS {
        dot11SMTbase2,
        dot11MACbase, dot11CountersGroup,
        dot11SmtAuthenticationAlgorithms, 
        dot11ResourceTypeID, dot11PhyOperationComplianceGroup }

   GROUP dot11PhyDSSSComplianceGroup
           DESCRIPTION
               "Implementation of this group is required when object
               dot11PHYType has the value of dsss.  This group is
               mutually exclusive with the groups
               dot11PhyIRComplianceGroup and
               dot11PhyFHSSComplianceGroup."

    GROUP dot11PhyIRComplianceGroup
           DESCRIPTION
               "Implementation of this group is required when object
               dot11PHYType has the value of irbaseband.  This group is
               mutually exclusive with the groups
               dot11PhyDSSSComplianceGroup and
               dot11PhyFHSSComplianceGroup."


    GROUP dot11PhyFHSSComplianceGroup
           DESCRIPTION
               "Implementation of this group is required when object
               dot11PHYType has the value of fhss.  This group is
               mutually exclusive with the groups
               dot11PhyDSSSComplianceGroup and
               dot11PhyIRComplianceGroup."


    -- OPTIONAL-GROUPS { dot11SMTprivacy, dot11MACStatistics,
    --    dot11PhyAntennaComplianceGroup, dot11PhyTxPowerComplianceGroup, 
    --    dot11PhyRegDomainsSupportGroup,
    --    dot11PhyAntennasListGroup, dot11PhyRateGroup }
    -- 

    ::= { dot11Compliances 1 }

-- **********************************************************************
-- *   Groups - units of conformance
-- **********************************************************************
dot11SMTbase OBJECT-GROUP
        OBJECTS { dot11StationID, dot11MediumOccupancyLimit, 
             dot11CFPollable,
             dot11CFPPeriod,
             dot11CFPMaxDuration,
             dot11AuthenticationResponseTimeOut,
             dot11PrivacyOptionImplemented,
             dot11PowerManagementMode,
             dot11DesiredSSID, dot11DesiredBSSType,
             dot11OperationalRateSet,
             dot11BeaconPeriod, dot11DTIMPeriod,
             dot11AssociationResponseTimeOut 
             }
        STATUS deprecated
        DESCRIPTION
         "The SMT object class provides the necessary support at the
         STA to manage the processes in the STA such that the STA may
         work cooperatively as a part of an IEEE 802.11 network."
    ::= {dot11Groups 1   }

dot11SMTprivacy OBJECT-GROUP
        OBJECTS { dot11PrivacyInvoked, 
                dot11WEPKeyMappingLength, dot11ExcludeUnencrypted,
                dot11WEPICVErrorCount , dot11WEPExcludedCount ,
                dot11WEPDefaultKeyID,
                dot11WEPDefaultKeyValue,
                dot11WEPKeyMappingWEPOn,
                dot11WEPKeyMappingValue , dot11WEPKeyMappingAddress,
                dot11WEPKeyMappingStatus }

        STATUS current
        DESCRIPTION
            "The SMTPrivacy package is a set of attributes that shall be
            present if WEP is implemented in the STA."
    ::= {dot11Groups 2 }

dot11MACbase OBJECT-GROUP

            OBJECTS { dot11MACAddress, dot11Address,
                    dot11GroupAddressesStatus,
                    dot11RTSThreshold, dot11ShortRetryLimit,
                    dot11LongRetryLimit, dot11FragmentationThreshold,
                    dot11MaxTransmitMSDULifetime,
                    dot11MaxReceiveLifetime, dot11ManufacturerID,
                    dot11ProductID
                    }
        STATUS current
        DESCRIPTION
         "The MAC object class provides the necessary support for the
         access control, generation, and verification of frame check
         sequences, and proper delivery of valid data to upper
         layers."
    ::= {dot11Groups 3 }


dot11MACStatistics OBJECT-GROUP

        OBJECTS { dot11RetryCount, dot11MultipleRetryCount,
            dot11RTSSuccessCount, dot11RTSFailureCount,
            dot11ACKFailureCount, dot11FrameDuplicateCount }

        STATUS current
        DESCRIPTION
            "The MACStatistics package provides extended statistical
            information on the operation of the MAC.  This 
            package is completely optional."
    ::= {dot11Groups 4 }

dot11ResourceTypeID OBJECT-GROUP
        OBJECTS { dot11ResourceTypeIDName, dot11manufacturerOUI,
            dot11manufacturerName, dot11manufacturerProductName,
            dot11manufacturerProductVersion }
        STATUS current
        DESCRIPTION

                "Attributes used to identify a STA, its manufacturer,
                and various product names and versions."

    ::= {dot11Groups 5  }

dot11SmtAuthenticationAlgorithms OBJECT-GROUP
        OBJECTS { dot11AuthenticationAlgorithm,
                  dot11AuthenticationAlgorithmsEnable }
        STATUS current
        DESCRIPTION
                "Authentication Algorithm Table."
    ::= {dot11Groups 6 }


dot11PhyOperationComplianceGroup OBJECT-GROUP
        OBJECTS { dot11PHYType, dot11CurrentRegDomain, dot11TempType }
        STATUS current
        DESCRIPTION
            "PHY layer operations attributes."
    ::= { dot11Groups 7 }


dot11PhyAntennaComplianceGroup OBJECT-GROUP
        OBJECTS {dot11CurrentTxAntenna, dot11DiversitySupport,
dot11CurrentRxAntenna }
        STATUS current
        DESCRIPTION
            "Attributes for Data Rates for IEEE 802.11."
    ::= { dot11Groups 8 }

dot11PhyTxPowerComplianceGroup OBJECT-GROUP
        OBJECTS {dot11NumberSupportedPowerLevels, dot11TxPowerLevel1,
            dot11TxPowerLevel2, dot11TxPowerLevel3, dot11TxPowerLevel4,
            dot11TxPowerLevel5, dot11TxPowerLevel6, dot11TxPowerLevel7,
            dot11TxPowerLevel8, dot11CurrentTxPowerLevel }
        STATUS current
        DESCRIPTION
            "Attributes for Control and Management of transmit power."
    ::= { dot11Groups 9 }

dot11PhyFHSSComplianceGroup OBJECT-GROUP
        OBJECTS {dot11HopTime, dot11CurrentChannelNumber, dot11MaxDwellTime,
            dot11CurrentDwellTime, dot11CurrentSet, dot11CurrentPattern,
            dot11CurrentIndex}

        STATUS current
        DESCRIPTION

            "Attributes that configure the Frequency Hopping for IEEE
            802.11."

    ::= { dot11Groups 10 }

dot11PhyDSSSComplianceGroup OBJECT-GROUP

        OBJECTS {dot11CurrentChannel, dot11CCAModeSupported,
            dot11CurrentCCAMode, dot11EDThreshold}

        STATUS current
        DESCRIPTION
            "Attributes that configure the DSSS for IEEE 802.11."
    ::= { dot11Groups 11 }

dot11PhyIRComplianceGroup OBJECT-GROUP
        OBJECTS {dot11CCAWatchdogTimerMax, dot11CCAWatchdogCountMax,
        dot11CCAWatchdogTimerMin, dot11CCAWatchdogCountMin}
        STATUS current
        DESCRIPTION
            "Attributes that configure the baseband IR for IEEE 802.11."
    ::= { dot11Groups 12 }

dot11PhyRegDomainsSupportGroup OBJECT-GROUP
        OBJECTS { dot11RegDomainsSupportValue}
        STATUS current
        DESCRIPTION
            "Attributes that specify the supported Regulation Domains."
    ::= { dot11Groups 13}

dot11PhyAntennasListGroup OBJECT-GROUP
        OBJECTS { dot11SupportedTxAntenna,
             dot11SupportedRxAntenna, dot11DiversitySelectionRx }
        STATUS current
        DESCRIPTION
            "Attributes that specify the supported Regulation Domains."
    ::= { dot11Groups 14 }

dot11PhyRateGroup OBJECT-GROUP
        OBJECTS {dot11SupportedDataRatesTxValue,
            dot11SupportedDataRatesRxValue }
        STATUS current
        DESCRIPTION
            "Attributes for Data Rates for IEEE 802.11."
    ::= { dot11Groups 15 }


dot11CountersGroup OBJECT-GROUP
        OBJECTS {  
                    dot11TransmittedFragmentCount   ,
                    dot11MulticastTransmittedFrameCount ,
                    dot11FailedCount, dot11ReceivedFragmentCount,
                    dot11MulticastReceivedFrameCount    ,
                    dot11FCSErrorCount,
                    dot11WEPUndecryptableCount,
                    dot11TransmittedFrameCount }

        STATUS current
        DESCRIPTION
            "Attributes from the dot11CountersGroup that are not described
            in the dot11MACStatistics group.  These objects are
            mandatory."
    ::= {dot11Groups 16 }

dot11NotificationGroup NOTIFICATION-GROUP
        NOTIFICATIONS { dot11Disassociate, 
                            dot11Deauthenticate,
                            dot11AuthenticateFail }
        STATUS current
        DESCRIPTION
                "IEEE 802.11 notifications"
        ::= { dot11Groups 17 }

dot11SMTbase2 OBJECT-GROUP
        OBJECTS { dot11MediumOccupancyLimit, 
             dot11CFPollable,
             dot11CFPPeriod,
             dot11CFPMaxDuration,
             dot11AuthenticationResponseTimeOut,
             dot11PrivacyOptionImplemented,
             dot11PowerManagementMode,
             dot11DesiredSSID, dot11DesiredBSSType,
             dot11OperationalRateSet,
             dot11BeaconPeriod, dot11DTIMPeriod,
             dot11AssociationResponseTimeOut,
             dot11DisassociateReason,
             dot11DisassociateStation,
             dot11DeauthenticateReason,
             dot11DeauthenticateStation,
             dot11AuthenticateFailStatus,
             dot11AuthenticateFailStation 
             }
        STATUS current
        DESCRIPTION
         "The SMTbase2 object class provides the necessary support at the
         STA to manage the processes in the STA such that the STA may
         work cooperatively as a part of an IEEE 802.11 network."
    ::= {dot11Groups 18 }

-- **********************************************************************
-- *   End of 80211 MIB
-- **********************************************************************
END
