When you've installed the driver, you must call the VBScript regmodify.vbs for each installed port:

cscript regmodify.vbs COM<x>

Replug the USB-CAN! Then you can open the port with any standard baudrate - except 115kbps! 

Take a look in the manual for more information.