

	 Content
	=========

The files in the folder of SNMP tools:

 Installation.txt		This file you are reading now
 .index				Sample entries for data in MIB index
 VSCOM.txt			The VScom MIB
 RS-232-MIB-rfc1659.txt		The RS232 MIB
 IEEE802dot11-MIB.txt		The WLAN MIB
 net-snmp-5.3.0.1-1.win32.exe	The installation program for SNMP tools


	 Installation of the software
	==============================

   1. Read the Net-SNMP.Readme.txt first.
   2. Install SNMP tools by executing net-snmp-5.3.0.1-1.win32.exe with the
      following steps.
   3. Select a target directory. "C:\Usr" is suggested by the installation
      program, may be any other directory.
   4. In the directory selected by the previous step there is a
      subdirectory %dir%\share\snmp\mibs, with a text file named ".index"
      in it.
   5. Open this file in a text editor (such as Notepad) and add these three
      lines to the file:
      IEEE802dot11-MIB IEEE802dot11-MIB.txt
      RS-232-MIB RS-232-MIB-rfc1659.txt
      VSCOM-MIB VSCOM.txt
      The file is alphabetically ordered, so use the appropriate positions.
   6. Save the file, make sure the name is still ".index".
   7. Copy the files IEEE802dot11-MIB.txt, RS-232-MIB-rfc1659.txt and
      VSCOM.txt to the same directory.
   8. If you wanna get rid of the prefix "VSCOM-MIB::" you must set an
      environment variable: "set MIBS=ALL"
   9. In case of doubt, restart your Windows.


	 Examples
	==========

snmpwalk -c public -v1 192.168.254.254 RS-232-MIB::rs232
snmpwalk -c public -v1 192.168.254.254 VSCOM-MIB::vsCom
snmpwalk -c public -v1 192.168.254.254 vsCom
snmpget -c public -v1 192.168.254.254 VSCOM-MIB::vsnciIpAddress.0
snmpwalk -c public -v1 192.168.254.254 system

# to reboot the NetCom (if you've set a password, you must replace the
# community "root" with this password)
snmpset -c root -v1 192.168.254.254 vsnciInternalControl.0 i 1

# set a new IpAddress
snmpset -c root -v1 192.168.254.254 vsnciIpAddress.0 a 192.168.1.1

192.168.254.254 is the default address of a NetCom server, replace this by
the IP address of your devices.